Micro CANopen Plus NXP MCUXpresso SDK Accelerator Demo
======================================================

VERSION:   0.90, EmSA 11-MAY-20
CONTACT:   info@esacademy.de


To operate this demo, you require:

1) MIMXRT1064-EVK board
   + with display installed
   + with CAN connector equipped (J11

2) LPC55S16-EVK board

3) USB cabling to operate the boards

4) Proper CAN cabling between CAN port of MIMXRT1064-EVK and LPC55S16-EVK
   + CAN_L, CAN_H and GND need to be connected between the boards
   + 120 Ohm terminaton resistors on both ends (between CAN_L, CAN_H)
     Note: on some LPC55S16-EVK boards this can be enabled by jumpers

	 
To operate the demo:
	 
Flash the provided demo code into the boards.
When boards are powered up, display shows X, Y and Z values coming from
the LPC55S16-EVK board. Move the LPC55S16-EVK to see theses values change.
On display, wipe up/down for different displays.
